Our commitment to sound excellence

The basic design of BMS high frequency drivers already offers enormous advantages,
providing 90% lower IM distortion than conventional dome drivers, as well as higher efficiency and phase linearity.
The High End (HE) modifications go one step ahead and raise the bar of audio performance even higher.

Selected materials, additional cooper shorting cups and modified phase-plugs make those transdusers
ultimately the best sounding devices available on the market.

Each driver is hand-selected to match +- 0.2dB tolerances, providing the best transducer choice for high resolution studio monitors,
high end home audio and superb cinema solutions.
The listener will experience the most dynamic performance and finest details never heard before.


The following models are available as High-End-Versions:

        4526HE 0.63" Neodymium HF Compression Driver, 1" VC, 25W AES, 113 dB

        4508HE 8" Dual Diaphragm Planar Wave Driver, 3.5" + 1.75" VC, 320 W + 80 W, 112 dB

        4593HE 1.4" Coaxial Neodymium compression driver, 3.5" + 1.75" VC, 150 W + 80 W, 118 dB

        4594HE 1.4" Coaxial Neodymium compression driver, 3.5" + 1.75" VC, 150 W + 80 W, 118 dB

        4595HE 1.5" Coaxial Neodymium compression driver, 3.5" + 1.75" VC, 150 W + 80 W, 118 dB

        4599HE 2" Dual Diaphragm Driver, 2x 3.5" VC, 400 W AES, 123 dB